HOW TO UPGRADE FIRMWARE

Make sure to save your calibration and other settings with SETUP Utility
-or- be prepared to do them over.  We strongly recommend that you
do an EE Reset after loading new firmware so the everything is initialized
the way the new firmware wants to see it.

v4 units firmware update is accomplished in SETUP Utility v4 using either RS-232 or USB.  

Click on "UPDATE FIRMWARE and follow the directions.




